{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Reparaturanforderung DE","Repair request EN"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Reparaturanforderung DE","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[[16,1,16,6],[22,1,22,6],[29,1,29,6],[14,4,14,6]]}
[]
[]
["Reparaturanforderung Befülladapter"]
[]
["Kunde"]
[null,"Name",null,null,"Telefon / Email"]
["Kontakt Instandhaltung"]
[]
["Adaptertyp",null,null,null,null,null,"Besonderheiten"]
[null,"Bremsfülladapter"]
[null,"Kühlerfülladapter"]
[null,"Twin AC HD"]
[null,"Twin AC ND"]
[]
["Seriennummer",null,null,null,"Medienleitung muss vor Anlieferung\nentleert und gereinigt werden."]
[]
["Fehlerbild"]
["Gewünschte Maßnahmen"]
[null,"Komplettservice Adapterkopf",null,null,"Austausch Adapterventile"]
[null,"Komplettservice Schlauchpaket",null,null,"Überholung Adapterventile"]
[null,"Wechsel Drucksensor"]
[null,"Wechsel Wegsensor"]
["Bemerkungen"]
[]
["Bereits ausgeführte Maßnahmen"]
[null,"Komplettservice Adapterkopf",null,null,"Austausch Adapterventile"]
[null,"Komplettservice Schlauchpaket",null,null,"Überholung Adapterventile"]
[null,"Wechsel Drucksensor"]
[null,"Wechsel Wegsensor"]
["Bemerkungen Maßnahmen"]
[]
["E-Mail Adressat 1","repair.somac@durr.com"]
["E-Mail Adressat 2"]
["E-Mail Adressat 3"]

{"sheet":"Repair request EN","index":1,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[[16,1,16,6],[22,1,22,6],[29,1,29,6],[14,4,14,6]]}
[]
[]
["Repair request Filling adapter"]
[]
["Customer"]
[null,"Name",null,null,"Telefon / Email"]
["Contact Maintenance"]
[]
["Adapter type",null,null,null,null,null,"Special"]
[null,"Brake Filling Adapter"]
[null,"Radiator Filling Adapter"]
[null,"Twin AC HP"]
[null,"Twin AC LP"]
[]
["Serial number",null,null,null,"Media pipe must be emptied \nand cleaned before shipment"]
[]
["Fault description"]
["Desired Services"]
[null,"Complete service adapter head",null,null,"Change adapter valves"]
[null,"Complete service hose package",null,null,"Seal change adapter valves"]
[null,"Change vac pressure sensor"]
[null,"Change nozzle possition system"]
["Remarks"]
[]
["Actions already taken by plant"]
[null,"Complete service adapter head",null,null,"Change adapter valves"]
[null,"Complete service hose package",null,null,"Seal change adapter valves"]
[null,"Change vac pressure sensor"]
[null,"Change nozzle possition system"]
["Remarks"]
[]
["E-Mail Adress 1","repair.somac@durr.com"]
["E-Mail Adress 2"]
["E-Mail Adress 3"]